Directions for the Waterfall Fountain

The pool Waterfall Fountain comes with 3 separate pieces that is easy to assemble.

Part A has an attached rotating head piece

Part B has a long neck connected to “L” shaped end piece

Part C is the waterfall piece

First you need to hold Part A rotating neck piece in your hand while inserting the long neck of Part B inside of Part A. Make sure Part B is tight inside of rubber piece inside of Part A and screwed tightly to ensure the neck is sturdy. Then hold the “L” shape of Part B as you insert Part C (the waterfall) inside of Part B. Make sure Part C is tighten inside of rubber piece and screwed onto Part B to ensure the waterfall is sturdy. Once all the pieces are assembled together you can connect Part A to the threaded return filter inside of the pool.